Supporting Information

for

Thermal conductivity performance of polypropylene composites filled with polydopamine-functionalized hexagonal boron nitride

Lin Chen1, Hong-Fei Xu1, Shao-Jian He2, Yi-Hang Du1, Nan-Jie Yu1,

Xiao-Ze Du1,\*, Jun Lin2,\*, Sergei Nazarenko3

1 Key Laboratory of Condition Monitoring and Control for Power Plant Equipment of Ministry of Education, North China Electric Power University, Beijing 102206, China

2 School of Renewable Energy, North China Electric Power University, Beijing 102206, China

3 School of Polymers and High Performance Materials, The University of Southern Mississippi, Hattiesburg, MS 39406, USA

\*Corresponding author 1: Xiao-Ze Du +86-10-61773923 duxz@ncepu.edu.cn

\*Corresponding author 2: Jun Lin +86-10-61772185 jun.lin@ncepu.edu.cn



S1 Fig. Thermal conductivity of the four series of polymer composites as a function of filler loading.