#

**S2 Fig. Monitoring of the production of the polyelectrolyte microcapsules by zeta potential measurement after each adsorption step**: Microcapsules were layered onto 6 µm CaCO3 particles. Error bars indicate the SD (n=3).