**S2 Fig. ImageJ analysis of standards run on the test card, blue channel.** Only the blue channel intensity was measured. The error bars are 1 SD of 3 replicate test zones. There is not good distinction at any time.