

Fig. S1. FTIR spectra of the produced olive mill solid waste-derived biochar (OMSW-BCs) (BC300: biochar produced at 300 °C; BC400: biochar produced at 400 °C; BC500: biochar produced at 500 °C; BC600: biochar produced at 600 °C; BC700: biochar produced at 700 °C).