**Fig S1. The receiver operating characteristic curve with the relative Youden’s index.**

The area under the curve with 4.8% cutoff point of %HA was 0.735. The sensitivity, the specificity, and the accuracy were 86.2%, 56.5%, and 73.1%, respectively). %HA = computed-tomography-derived %honeycombing area.