|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Minimum slice thickness with sinc RF pulse  (time-bandwidth product = 6000 Hz\*ms) | | | |
| Maximum gradient strength | RF pulse duration = 0.5 ms | RF pulse duration = 1 ms | RF pulse duration = 2 ms | RF pulse duration = 4 ms |
| 40 mT/m | 7.04 mm | 3.52 mm | 1.76 mm | 0.88 mm |
| 80 mT/m | 3.52 mm | 1.76 mm | 0.88 mm | 0.44 mm |
| 675 mT/m | 0.42 mm | 0.21 mm | 0.10 mm | 0.05 mm |