**S1 Table. ATLIS Controlcommands**

|  |  |
| --- | --- |
| **COMMAND** | **FUNCTION** |
| T | Set target temperature |
| C | Set controlling temperature sensor |
| L | Set limiting temperature sensor |
| M | Set heating unit maximum temperature |
| P | Set KP value |
| I | Set KI value |
| D | Set KD value |
| W | Set time between temperature recordings |
| S | Set shutter position |
| R 1 | Request a temperature read |
| R 2 | Request full system settings |